
# Copyright (C) 2017-2018 Daniel Tartavel-jeannot   <dtux@free.fr>
#
# This program is free software; you can redistribute it and/or modify
# it under the terms of the GNU General Public License as published by
# the Free Software Foundation; either version 2 of the License, or
# (at your option) any later version.
#
# This program is distributed in the hope that it will be useful,
# but WITHOUT ANY WARRANTY; without even the implied warranty of
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
# GNU General Public License for more details.
#
# You should have received a copy of the GNU General Public License
# along with this program. If not, see <http://www.gnu.org/licenses/>.


MAGEIA_VERSION="7"
ARM_VERSION="armv7hl"

#target plateform (xu3-4 or rpi)
TARGET="rpi"
#version of the target
# 0, 1, 2 ,3_32 for rpi and 3 or 4 for odroid
TARGET_VERSION="3_32"

# URL of the Mageia mirror used to install ( see mirrors.mageia.org )
MIRROR="http://ftp.free.fr/mirrors/mageia.org/distrib/$MAGEIA_VERSION/$ARM_VERSION"
# image will be created here
INSTALL_PATH="<change this>"

# Build directory will be created here
BUILD_PATH="$INSTALL_PATH/build"

#name of the image
IMAGE="Mageia-${MAGEIA_VERSION}-$TARGET.img"

#Mount point of image's partitions
#no need to be changed
BOOT="/mnt/boot"
ROOT="/mnt/root"

#Default user
ID_USER="pi"
PASSWORD="raspberry"

#root password
ROOT_PWD="piroot"

#Hostname
HOSTNAME="$TARGET.$ID_USER"

#Filesystem of boot partitions (default ext4 raspberry pi need vfat)
#DO NOT CHANGE THIS
BOOTFS="vfat"

#Path where the raspberry pi firmware is/will be installed
FIRMWARE_PATH="$INSTALL_PATH"
FIRMWARE_DIR="firmware-stable"
